commit 9884107af289f8a441156b7a7eff73c39e74467e
Author: Nicolas Chauvet <kwizart@gmail.com>
Date:   Wed Mar 27 18:01:43 2024 +0100

    Add redhat patches

diff --git a/arch/s390/include/asm/ipl.h b/arch/s390/include/asm/ipl.h
index b0d00032479d..afb9544fb007 100644
--- a/arch/s390/include/asm/ipl.h
+++ b/arch/s390/include/asm/ipl.h
@@ -139,6 +139,7 @@ int ipl_report_add_component(struct ipl_report *report, struct kexec_buf *kbuf,
 			     unsigned char flags, unsigned short cert);
 int ipl_report_add_certificate(struct ipl_report *report, void *key,
 			       unsigned long addr, unsigned long len);
+bool ipl_get_secureboot(void);
 
 /*
  * DIAG 308 support
diff --git a/arch/s390/kernel/ipl.c b/arch/s390/kernel/ipl.c
index 8d0b95c17312..118ae555a179 100644
--- a/arch/s390/kernel/ipl.c
+++ b/arch/s390/kernel/ipl.c
@@ -2520,3 +2520,8 @@ int ipl_report_free(struct ipl_report *report)
 }
 
 #endif
+
+bool ipl_get_secureboot(void)
+{
+	return !!ipl_secure_flag;
+}
diff --git a/arch/s390/kernel/setup.c b/arch/s390/kernel/setup.c
index de6ad0fb2328..5cc2758be027 100644
--- a/arch/s390/kernel/setup.c
+++ b/arch/s390/kernel/setup.c
@@ -49,6 +49,7 @@
 #include <linux/memory.h>
 #include <linux/compat.h>
 #include <linux/start_kernel.h>
+#include <linux/security.h>
 #include <linux/hugetlb.h>
 #include <linux/kmemleak.h>
 
@@ -914,6 +915,9 @@ void __init setup_arch(char **cmdline_p)
 
 	log_component_list();
 
+	if (ipl_get_secureboot())
+		security_lock_kernel_down("Secure IPL mode", LOCKDOWN_INTEGRITY_MAX);
+
 	/* Have one command line that is parsed and saved in /proc/cmdline */
 	/* boot_command_line has been already set up in early.c */
 	*cmdline_p = boot_command_line;
diff --git a/arch/x86/kernel/setup.c b/arch/x86/kernel/setup.c
index e63a8d05ce29..92700cd1048e 100644
--- a/arch/x86/kernel/setup.c
+++ b/arch/x86/kernel/setup.c
@@ -20,6 +20,7 @@
 #include <linux/root_dev.h>
 #include <linux/hugetlb.h>
 #include <linux/tboot.h>
+#include <linux/security.h>
 #include <linux/usb/xhci-dbgp.h>
 #include <linux/static_call.h>
 #include <linux/swiotlb.h>
@@ -1027,6 +1028,13 @@ void __init setup_arch(char **cmdline_p)
 	if (efi_enabled(EFI_BOOT))
 		efi_init();
 
+	efi_set_secure_boot(boot_params.secure_boot);
+
+#ifdef CONFIG_LOCK_DOWN_IN_EFI_SECURE_BOOT
+	if (efi_enabled(EFI_SECURE_BOOT))
+		security_lock_kernel_down("EFI Secure Boot mode", LOCKDOWN_INTEGRITY_MAX);
+#endif
+
 	reserve_ibft_region();
 	x86_init.resources.dmi_setup();
 
@@ -1188,19 +1196,7 @@ void __init setup_arch(char **cmdline_p)
 	/* Allocate bigger log buffer */
 	setup_log_buf(1);
 
-	if (efi_enabled(EFI_BOOT)) {
-		switch (boot_params.secure_boot) {
-		case efi_secureboot_mode_disabled:
-			pr_info("Secure boot disabled\n");
-			break;
-		case efi_secureboot_mode_enabled:
-			pr_info("Secure boot enabled\n");
-			break;
-		default:
-			pr_info("Secure boot could not be determined\n");
-			break;
-		}
-	}
+	efi_set_secure_boot(boot_params.secure_boot);
 
 	reserve_initrd();
 
diff --git a/drivers/acpi/apei/hest.c b/drivers/acpi/apei/hest.c
index 6aef1ee5e1bd..8f146b1b4972 100644
--- a/drivers/acpi/apei/hest.c
+++ b/drivers/acpi/apei/hest.c
@@ -96,6 +96,14 @@ static int apei_hest_parse(apei_hest_func_t func, void *data)
 	if (hest_disable || !hest_tab)
 		return -EINVAL;
 
+#ifdef CONFIG_ARM64
+	/* Ignore broken firmware */
+	if (!strncmp(hest_tab->header.oem_id, "HPE   ", 6) &&
+	    !strncmp(hest_tab->header.oem_table_id, "ProLiant", 8) &&
+	    MIDR_IMPLEMENTOR(read_cpuid_id()) == ARM_CPU_IMP_APM)
+		return -EINVAL;
+#endif
+
 	hest_hdr = (struct acpi_hest_header *)(hest_tab + 1);
 	for (i = 0; i < hest_tab->error_source_count; i++) {
 		len = hest_esrc_len(hest_hdr);
diff --git a/drivers/acpi/irq.c b/drivers/acpi/irq.c
index 1687483ff319..390b67f19181 100644
--- a/drivers/acpi/irq.c
+++ b/drivers/acpi/irq.c
@@ -143,6 +143,7 @@ struct acpi_irq_parse_one_ctx {
 	unsigned int index;
 	unsigned long *res_flags;
 	struct irq_fwspec *fwspec;
+	bool skip_producer_check;
 };
 
 /**
@@ -216,7 +217,8 @@ static acpi_status acpi_irq_parse_one_cb(struct acpi_resource *ares,
 		return AE_CTRL_TERMINATE;
 	case ACPI_RESOURCE_TYPE_EXTENDED_IRQ:
 		eirq = &ares->data.extended_irq;
-		if (eirq->producer_consumer == ACPI_PRODUCER)
+		if (!ctx->skip_producer_check &&
+		    eirq->producer_consumer == ACPI_PRODUCER)
 			return AE_OK;
 		if (ctx->index >= eirq->interrupt_count) {
 			ctx->index -= eirq->interrupt_count;
@@ -252,8 +254,19 @@ static acpi_status acpi_irq_parse_one_cb(struct acpi_resource *ares,
 static int acpi_irq_parse_one(acpi_handle handle, unsigned int index,
 			      struct irq_fwspec *fwspec, unsigned long *flags)
 {
-	struct acpi_irq_parse_one_ctx ctx = { -EINVAL, index, flags, fwspec };
+	struct acpi_irq_parse_one_ctx ctx = { -EINVAL, index, flags, fwspec, false };
 
+	/*
+	 * Firmware on arm64-based HPE m400 platform incorrectly marks
+	 * its UART interrupt as ACPI_PRODUCER rather than ACPI_CONSUMER.
+	 * Don't do the producer/consumer check for that device.
+	 */
+	if (IS_ENABLED(CONFIG_ARM64)) {
+		struct acpi_device *adev = acpi_get_acpi_dev(handle);
+
+		if (adev && !strcmp(acpi_device_hid(adev), "APMC0D08"))
+			ctx.skip_producer_check = true;
+	}
 	acpi_walk_resources(handle, METHOD_NAME__CRS, acpi_irq_parse_one_cb, &ctx);
 	return ctx.rc;
 }
diff --git a/drivers/acpi/scan.c b/drivers/acpi/scan.c
index 597d75baa1cc..ee38441143bf 100644
--- a/drivers/acpi/scan.c
+++ b/drivers/acpi/scan.c
@@ -1753,6 +1753,15 @@ static bool acpi_device_enumeration_by_parent(struct acpi_device *device)
 	if (!acpi_match_device_ids(device, ignore_serial_bus_ids))
 		return false;
 
+	/*
+	 * Firmware on some arm64 X-Gene platforms will make the UART
+	 * device appear as both a UART and a slave of that UART. Just
+	 * bail out here for X-Gene UARTs.
+	 */
+	if (IS_ENABLED(CONFIG_ARM64) &&
+	    !strcmp(acpi_device_hid(device), "APMC0D08"))
+		return false;
+
 	INIT_LIST_HEAD(&resource_list);
 	acpi_dev_get_resources(device, &resource_list,
 			       acpi_check_serial_bus_slave,
diff --git a/drivers/ata/libahci.c b/drivers/ata/libahci.c
index f1263364fa97..24ac410f4366 100644
--- a/drivers/ata/libahci.c
+++ b/drivers/ata/libahci.c
@@ -729,6 +729,24 @@ int ahci_stop_engine(struct ata_port *ap)
 	tmp &= ~PORT_CMD_START;
 	writel(tmp, port_mmio + PORT_CMD);
 
+#ifdef CONFIG_ARM64
+	/* Rev Ax of Cavium CN99XX needs a hack for port stop */
+	if (dev_is_pci(ap->host->dev) &&
+	    to_pci_dev(ap->host->dev)->vendor == 0x14e4 &&
+	    to_pci_dev(ap->host->dev)->device == 0x9027 &&
+	    midr_is_cpu_model_range(read_cpuid_id(),
+			MIDR_CPU_MODEL(ARM_CPU_IMP_BRCM, BRCM_CPU_PART_VULCAN),
+			MIDR_CPU_VAR_REV(0, 0),
+			MIDR_CPU_VAR_REV(0, MIDR_REVISION_MASK))) {
+		tmp = readl(hpriv->mmio + 0x8000);
+		udelay(100);
+		writel(tmp | (1 << 26), hpriv->mmio + 0x8000);
+		udelay(100);
+		writel(tmp & ~(1 << 26), hpriv->mmio + 0x8000);
+		dev_warn(ap->host->dev, "CN99XX SATA reset workaround applied\n");
+	}
+#endif
+
 	/* wait for engine to stop. This could be as long as 500 msec */
 	tmp = ata_wait_register(ap, port_mmio + PORT_CMD,
 				PORT_CMD_LIST_ON, PORT_CMD_LIST_ON, 1, 500);
diff --git a/drivers/char/ipmi/ipmi_dmi.c b/drivers/char/ipmi/ipmi_dmi.c
index bbf7029e224b..cf7faa970dd6 100644
--- a/drivers/char/ipmi/ipmi_dmi.c
+++ b/drivers/char/ipmi/ipmi_dmi.c
@@ -215,6 +215,21 @@ static int __init scan_for_dmi_ipmi(void)
 {
 	const struct dmi_device *dev = NULL;
 
+#ifdef CONFIG_ARM64
+	/* RHEL-only
+	 * If this is ARM-based HPE m400, return now, because that platform
+	 * reports the host-side ipmi address as intel port-io space, which
+	 * does not exist in the ARM architecture.
+	 */
+	const char *dmistr = dmi_get_system_info(DMI_PRODUCT_NAME);
+
+	if (dmistr && (strcmp("ProLiant m400 Server", dmistr) == 0)) {
+		pr_debug("%s does not support host ipmi\n", dmistr);
+		return 0;
+	}
+	/* END RHEL-only */
+#endif
+
 	while ((dev = dmi_find_device(DMI_DEV_TYPE_IPMI, NULL, dev)))
 		dmi_decode_ipmi((const struct dmi_header *) dev->device_data);
 
diff --git a/drivers/char/ipmi/ipmi_msghandler.c b/drivers/char/ipmi/ipmi_msghandler.c
index 186f1fee7534..93e3a76596ff 100644
--- a/drivers/char/ipmi/ipmi_msghandler.c
+++ b/drivers/char/ipmi/ipmi_msghandler.c
@@ -35,6 +35,7 @@
 #include <linux/uuid.h>
 #include <linux/nospec.h>
 #include <linux/vmalloc.h>
+#include <linux/dmi.h>
 #include <linux/delay.h>
 
 #define IPMI_DRIVER_VERSION "39.2"
@@ -5516,8 +5517,21 @@ static int __init ipmi_init_msghandler_mod(void)
 {
 	int rv;
 
-	pr_info("version " IPMI_DRIVER_VERSION "\n");
+#ifdef CONFIG_ARM64
+	/* RHEL-only
+	 * If this is ARM-based HPE m400, return now, because that platform
+	 * reports the host-side ipmi address as intel port-io space, which
+	 * does not exist in the ARM architecture.
+	 */
+	const char *dmistr = dmi_get_system_info(DMI_PRODUCT_NAME);
 
+	if (dmistr && (strcmp("ProLiant m400 Server", dmistr) == 0)) {
+		pr_debug("%s does not support host ipmi\n", dmistr);
+		return -ENOSYS;
+	}
+	/* END RHEL-only */
+#endif
+	pr_info("version " IPMI_DRIVER_VERSION "\n");
 	mutex_lock(&ipmi_interfaces_mutex);
 	rv = ipmi_register_driver();
 	mutex_unlock(&ipmi_interfaces_mutex);
diff --git a/drivers/firmware/efi/Makefile b/drivers/firmware/efi/Makefile
index e489fefd23da..f2dfae764fb5 100644
--- a/drivers/firmware/efi/Makefile
+++ b/drivers/firmware/efi/Makefile
@@ -25,6 +25,7 @@ subdir-$(CONFIG_EFI_STUB)		+= libstub
 obj-$(CONFIG_EFI_BOOTLOADER_CONTROL)	+= efibc.o
 obj-$(CONFIG_EFI_TEST)			+= test/
 obj-$(CONFIG_EFI_DEV_PATH_PARSER)	+= dev-path-parser.o
+obj-$(CONFIG_EFI)			+= secureboot.o
 obj-$(CONFIG_APPLE_PROPERTIES)		+= apple-properties.o
 obj-$(CONFIG_EFI_RCI2_TABLE)		+= rci2-table.o
 obj-$(CONFIG_EFI_EMBEDDED_FIRMWARE)	+= embedded-firmware.o
diff --git a/drivers/firmware/efi/efi.c b/drivers/firmware/efi/efi.c
index 2c1095dcc2f2..7ea6012e3ef4 100644
--- a/drivers/firmware/efi/efi.c
+++ b/drivers/firmware/efi/efi.c
@@ -32,6 +32,7 @@
 #include <linux/ucs2_string.h>
 #include <linux/memblock.h>
 #include <linux/security.h>
+#include <linux/bsearch.h>
 
 #include <asm/early_ioremap.h>
 
@@ -985,40 +986,101 @@ int efi_mem_type(unsigned long phys_addr)
 }
 #endif
 
+struct efi_error_code {
+	efi_status_t status;
+	int errno;
+	const char *description;
+};
+
+static const struct efi_error_code efi_error_codes[] = {
+	{ EFI_SUCCESS, 0, "Success"},
+#if 0
+	{ EFI_LOAD_ERROR, -EPICK_AN_ERRNO, "Load Error"},
+#endif
+	{ EFI_INVALID_PARAMETER, -EINVAL, "Invalid Parameter"},
+	{ EFI_UNSUPPORTED, -ENOSYS, "Unsupported"},
+	{ EFI_BAD_BUFFER_SIZE, -ENOSPC, "Bad Buffer Size"},
+	{ EFI_BUFFER_TOO_SMALL, -ENOSPC, "Buffer Too Small"},
+	{ EFI_NOT_READY, -EAGAIN, "Not Ready"},
+	{ EFI_DEVICE_ERROR, -EIO, "Device Error"},
+	{ EFI_WRITE_PROTECTED, -EROFS, "Write Protected"},
+	{ EFI_OUT_OF_RESOURCES, -ENOMEM, "Out of Resources"},
+#if 0
+	{ EFI_VOLUME_CORRUPTED, -EPICK_AN_ERRNO, "Volume Corrupt"},
+	{ EFI_VOLUME_FULL, -EPICK_AN_ERRNO, "Volume Full"},
+	{ EFI_NO_MEDIA, -EPICK_AN_ERRNO, "No Media"},
+	{ EFI_MEDIA_CHANGED, -EPICK_AN_ERRNO, "Media changed"},
+#endif
+	{ EFI_NOT_FOUND, -ENOENT, "Not Found"},
+#if 0
+	{ EFI_ACCESS_DENIED, -EPICK_AN_ERRNO, "Access Denied"},
+	{ EFI_NO_RESPONSE, -EPICK_AN_ERRNO, "No Response"},
+	{ EFI_NO_MAPPING, -EPICK_AN_ERRNO, "No mapping"},
+	{ EFI_TIMEOUT, -EPICK_AN_ERRNO, "Time out"},
+	{ EFI_NOT_STARTED, -EPICK_AN_ERRNO, "Not started"},
+	{ EFI_ALREADY_STARTED, -EPICK_AN_ERRNO, "Already started"},
+#endif
+	{ EFI_ABORTED, -EINTR, "Aborted"},
+#if 0
+	{ EFI_ICMP_ERROR, -EPICK_AN_ERRNO, "ICMP Error"},
+	{ EFI_TFTP_ERROR, -EPICK_AN_ERRNO, "TFTP Error"},
+	{ EFI_PROTOCOL_ERROR, -EPICK_AN_ERRNO, "Protocol Error"},
+	{ EFI_INCOMPATIBLE_VERSION, -EPICK_AN_ERRNO, "Incompatible Version"},
+#endif
+	{ EFI_SECURITY_VIOLATION, -EACCES, "Security Policy Violation"},
+#if 0
+	{ EFI_CRC_ERROR, -EPICK_AN_ERRNO, "CRC Error"},
+	{ EFI_END_OF_MEDIA, -EPICK_AN_ERRNO, "End of Media"},
+	{ EFI_END_OF_FILE, -EPICK_AN_ERRNO, "End of File"},
+	{ EFI_INVALID_LANGUAGE, -EPICK_AN_ERRNO, "Invalid Languages"},
+	{ EFI_COMPROMISED_DATA, -EPICK_AN_ERRNO, "Compromised Data"},
+
+	// warnings
+	{ EFI_WARN_UNKOWN_GLYPH, -EPICK_AN_ERRNO, "Warning Unknown Glyph"},
+	{ EFI_WARN_DELETE_FAILURE, -EPICK_AN_ERRNO, "Warning Delete Failure"},
+	{ EFI_WARN_WRITE_FAILURE, -EPICK_AN_ERRNO, "Warning Write Failure"},
+	{ EFI_WARN_BUFFER_TOO_SMALL, -EPICK_AN_ERRNO, "Warning Buffer Too Small"},
+#endif
+};
+
+static int
+efi_status_cmp_bsearch(const void *key, const void *item)
+{
+	u64 status = (u64)(uintptr_t)key;
+	struct efi_error_code *code = (struct efi_error_code *)item;
+
+	if (status < code->status)
+		return -1;
+	if (status > code->status)
+		return 1;
+	return 0;
+}
+
 int efi_status_to_err(efi_status_t status)
 {
-	int err;
-
-	switch (status) {
-	case EFI_SUCCESS:
-		err = 0;
-		break;
-	case EFI_INVALID_PARAMETER:
-		err = -EINVAL;
-		break;
-	case EFI_OUT_OF_RESOURCES:
-		err = -ENOSPC;
-		break;
-	case EFI_DEVICE_ERROR:
-		err = -EIO;
-		break;
-	case EFI_WRITE_PROTECTED:
-		err = -EROFS;
-		break;
-	case EFI_SECURITY_VIOLATION:
-		err = -EACCES;
-		break;
-	case EFI_NOT_FOUND:
-		err = -ENOENT;
-		break;
-	case EFI_ABORTED:
-		err = -EINTR;
-		break;
-	default:
-		err = -EINVAL;
-	}
+	struct efi_error_code *found;
+	size_t num = sizeof(efi_error_codes) / sizeof(struct efi_error_code);
 
-	return err;
+	found = bsearch((void *)(uintptr_t)status, efi_error_codes,
+			sizeof(struct efi_error_code), num,
+			efi_status_cmp_bsearch);
+	if (!found)
+		return -EINVAL;
+	return found->errno;
+}
+
+const char *
+efi_status_to_str(efi_status_t status)
+{
+	struct efi_error_code *found;
+	size_t num = sizeof(efi_error_codes) / sizeof(struct efi_error_code);
+
+	found = bsearch((void *)(uintptr_t)status, efi_error_codes,
+			sizeof(struct efi_error_code), num,
+			efi_status_cmp_bsearch);
+	if (!found)
+		return "Unknown error code";
+	return found->description;
 }
 EXPORT_SYMBOL_GPL(efi_status_to_err);
 
diff --git a/drivers/firmware/efi/secureboot.c b/drivers/firmware/efi/secureboot.c
new file mode 100644
index 000000000000..de0a3714a5d4
--- /dev/null
+++ b/drivers/firmware/efi/secureboot.c
@@ -0,0 +1,38 @@
+/* Core kernel secure boot support.
+ *
+ * Copyright (C) 2017 Red Hat, Inc. All Rights Reserved.
+ * Written by David Howells (dhowells@redhat.com)
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public Licence
+ * as published by the Free Software Foundation; either version
+ * 2 of the Licence, or (at your option) any later version.
+ */
+
+#define pr_fmt(fmt) KBUILD_MODNAME ": " fmt
+
+#include <linux/efi.h>
+#include <linux/kernel.h>
+#include <linux/printk.h>
+
+/*
+ * Decide what to do when UEFI secure boot mode is enabled.
+ */
+void __init efi_set_secure_boot(enum efi_secureboot_mode mode)
+{
+	if (efi_enabled(EFI_BOOT)) {
+		switch (mode) {
+		case efi_secureboot_mode_disabled:
+			pr_info("Secure boot disabled\n");
+			break;
+		case efi_secureboot_mode_enabled:
+			set_bit(EFI_SECURE_BOOT, &efi.flags);
+			pr_info("Secure boot enabled\n");
+			break;
+		default:
+			pr_warn("Secure boot could not be determined (mode %u)\n",
+				   mode);
+			break;
+		}
+	}
+}
diff --git a/drivers/firmware/sysfb.c b/drivers/firmware/sysfb.c
index 3c197db42c9d..16e4a2e90fae 100644
--- a/drivers/firmware/sysfb.c
+++ b/drivers/firmware/sysfb.c
@@ -34,6 +34,22 @@
 #include <linux/screen_info.h>
 #include <linux/sysfb.h>
 
+static int skip_simpledrm;
+
+static int __init simpledrm_disable(char *opt)
+{
+	if (!opt)
+                return -EINVAL;
+
+	get_option(&opt, &skip_simpledrm);
+
+	if (skip_simpledrm)
+		pr_info("The simpledrm driver will not be probed\n");
+
+	return 0;
+}
+early_param("nvidia-drm.modeset", simpledrm_disable);
+
 static struct platform_device *pd;
 static DEFINE_MUTEX(disable_lock);
 static bool disabled;
@@ -85,7 +101,7 @@ static __init int sysfb_init(void)
 
 	/* try to create a simple-framebuffer device */
 	compatible = sysfb_parse_mode(si, &mode);
-	if (compatible) {
+	if (compatible && !skip_simpledrm) {
 		pd = sysfb_create_simplefb(si, &mode);
 		if (!IS_ERR(pd))
 			goto unlock_mutex;
diff --git a/drivers/hid/hid-rmi.c b/drivers/hid/hid-rmi.c
index 84e7ba5314d3..efc96776f761 100644
--- a/drivers/hid/hid-rmi.c
+++ b/drivers/hid/hid-rmi.c
@@ -321,21 +321,12 @@ static int rmi_input_event(struct hid_device *hdev, u8 *data, int size)
 {
 	struct rmi_data *hdata = hid_get_drvdata(hdev);
 	struct rmi_device *rmi_dev = hdata->xport.rmi_dev;
-	unsigned long flags;
 
 	if (!(test_bit(RMI_STARTED, &hdata->flags)))
 		return 0;
 
-	pm_wakeup_event(hdev->dev.parent, 0);
-
-	local_irq_save(flags);
-
 	rmi_set_attn_data(rmi_dev, data[1], &data[2], size - 2);
 
-	generic_handle_irq(hdata->rmi_irq);
-
-	local_irq_restore(flags);
-
 	return 1;
 }
 
@@ -591,56 +582,6 @@ static const struct rmi_transport_ops hid_rmi_ops = {
 	.reset		= rmi_hid_reset,
 };
 
-static void rmi_irq_teardown(void *data)
-{
-	struct rmi_data *hdata = data;
-	struct irq_domain *domain = hdata->domain;
-
-	if (!domain)
-		return;
-
-	irq_dispose_mapping(irq_find_mapping(domain, 0));
-
-	irq_domain_remove(domain);
-	hdata->domain = NULL;
-	hdata->rmi_irq = 0;
-}
-
-static int rmi_irq_map(struct irq_domain *h, unsigned int virq,
-		       irq_hw_number_t hw_irq_num)
-{
-	irq_set_chip_and_handler(virq, &dummy_irq_chip, handle_simple_irq);
-
-	return 0;
-}
-
-static const struct irq_domain_ops rmi_irq_ops = {
-	.map = rmi_irq_map,
-};
-
-static int rmi_setup_irq_domain(struct hid_device *hdev)
-{
-	struct rmi_data *hdata = hid_get_drvdata(hdev);
-	int ret;
-
-	hdata->domain = irq_domain_create_linear(hdev->dev.fwnode, 1,
-						 &rmi_irq_ops, hdata);
-	if (!hdata->domain)
-		return -ENOMEM;
-
-	ret = devm_add_action_or_reset(&hdev->dev, &rmi_irq_teardown, hdata);
-	if (ret)
-		return ret;
-
-	hdata->rmi_irq = irq_create_mapping(hdata->domain, 0);
-	if (hdata->rmi_irq <= 0) {
-		hid_err(hdev, "Can't allocate an IRQ\n");
-		return hdata->rmi_irq < 0 ? hdata->rmi_irq : -ENXIO;
-	}
-
-	return 0;
-}
-
 static int rmi_probe(struct hid_device *hdev, const struct hid_device_id *id)
 {
 	struct rmi_data *data = NULL;
@@ -713,18 +654,11 @@ static int rmi_probe(struct hid_device *hdev, const struct hid_device_id *id)
 
 	mutex_init(&data->page_mutex);
 
-	ret = rmi_setup_irq_domain(hdev);
-	if (ret) {
-		hid_err(hdev, "failed to allocate IRQ domain\n");
-		return ret;
-	}
-
 	if (data->device_flags & RMI_DEVICE_HAS_PHYS_BUTTONS)
 		rmi_hid_pdata.gpio_data.disable = true;
 
 	data->xport.dev = hdev->dev.parent;
 	data->xport.pdata = rmi_hid_pdata;
-	data->xport.pdata.irq = data->rmi_irq;
 	data->xport.proto_name = "hid";
 	data->xport.ops = &hid_rmi_ops;
 
diff --git a/drivers/hwtracing/coresight/coresight-etm4x-core.c b/drivers/hwtracing/coresight/coresight-etm4x-core.c
index 18c4544f6045..4c37cdc40426 100644
--- a/drivers/hwtracing/coresight/coresight-etm4x-core.c
+++ b/drivers/hwtracing/coresight/coresight-etm4x-core.c
@@ -10,6 +10,7 @@
 #include <linux/init.h>
 #include <linux/types.h>
 #include <linux/device.h>
+#include <linux/dmi.h>
 #include <linux/io.h>
 #include <linux/err.h>
 #include <linux/fs.h>
@@ -2303,6 +2304,16 @@ static const struct amba_id etm4_ids[] = {
 	{},
 };
 
+static const struct dmi_system_id broken_coresight[] = {
+	{
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "HPE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "Apollo 70"),
+		},
+	},
+	{ }	/* terminating entry */
+};
+
 MODULE_DEVICE_TABLE(amba, etm4_ids);
 
 static struct amba_driver etm4x_amba_driver = {
@@ -2372,6 +2383,11 @@ static int __init etm4x_init(void)
 {
 	int ret;
 
+	if (dmi_check_system(broken_coresight)) {
+		pr_info("ETM4 disabled due to firmware bug\n");
+		return 0;
+	}
+
 	ret = etm4_pm_setup();
 
 	/* etm4_pm_setup() does its own cleanup - exit on error */
@@ -2398,6 +2414,9 @@ static int __init etm4x_init(void)
 
 static void __exit etm4x_exit(void)
 {
+	if (dmi_check_system(broken_coresight))
+		return;
+
 	amba_driver_unregister(&etm4x_amba_driver);
 	platform_driver_unregister(&etm4_platform_driver);
 	etm4_pm_clear();
diff --git a/drivers/input/rmi4/rmi_driver.c b/drivers/input/rmi4/rmi_driver.c
index 258d5fe3d395..f7298e3dc8f3 100644
--- a/drivers/input/rmi4/rmi_driver.c
+++ b/drivers/input/rmi4/rmi_driver.c
@@ -182,34 +182,47 @@ void rmi_set_attn_data(struct rmi_device *rmi_dev, unsigned long irq_status,
 	attn_data.data = fifo_data;
 
 	kfifo_put(&drvdata->attn_fifo, attn_data);
+
+	schedule_work(&drvdata->attn_work);
 }
 EXPORT_SYMBOL_GPL(rmi_set_attn_data);
 
-static irqreturn_t rmi_irq_fn(int irq, void *dev_id)
+static void attn_callback(struct work_struct *work)
 {
-	struct rmi_device *rmi_dev = dev_id;
-	struct rmi_driver_data *drvdata = dev_get_drvdata(&rmi_dev->dev);
+	struct rmi_driver_data *drvdata = container_of(work,
+							struct rmi_driver_data,
+							attn_work);
 	struct rmi4_attn_data attn_data = {0};
 	int ret, count;
 
 	count = kfifo_get(&drvdata->attn_fifo, &attn_data);
-	if (count) {
-		*(drvdata->irq_status) = attn_data.irq_status;
-		drvdata->attn_data = attn_data;
-	}
+	if (!count)
+		return;
 
-	ret = rmi_process_interrupt_requests(rmi_dev);
+	*(drvdata->irq_status) = attn_data.irq_status;
+	drvdata->attn_data = attn_data;
+
+	ret = rmi_process_interrupt_requests(drvdata->rmi_dev);
 	if (ret)
-		rmi_dbg(RMI_DEBUG_CORE, &rmi_dev->dev,
+		rmi_dbg(RMI_DEBUG_CORE, &drvdata->rmi_dev->dev,
 			"Failed to process interrupt request: %d\n", ret);
 
-	if (count) {
-		kfree(attn_data.data);
-		drvdata->attn_data.data = NULL;
-	}
+	kfree(attn_data.data);
+	drvdata->attn_data.data = NULL;
 
 	if (!kfifo_is_empty(&drvdata->attn_fifo))
-		return rmi_irq_fn(irq, dev_id);
+		schedule_work(&drvdata->attn_work);
+}
+
+static irqreturn_t rmi_irq_fn(int irq, void *dev_id)
+{
+	struct rmi_device *rmi_dev = dev_id;
+	int ret;
+
+	ret = rmi_process_interrupt_requests(rmi_dev);
+	if (ret)
+		rmi_dbg(RMI_DEBUG_CORE, &rmi_dev->dev,
+			"Failed to process interrupt request: %d\n", ret);
 
 	return IRQ_HANDLED;
 }
@@ -217,7 +230,6 @@ static irqreturn_t rmi_irq_fn(int irq, void *dev_id)
 static int rmi_irq_init(struct rmi_device *rmi_dev)
 {
 	struct rmi_device_platform_data *pdata = rmi_get_platform_data(rmi_dev);
-	struct rmi_driver_data *data = dev_get_drvdata(&rmi_dev->dev);
 	int irq_flags = irq_get_trigger_type(pdata->irq);
 	int ret;
 
@@ -235,8 +247,6 @@ static int rmi_irq_init(struct rmi_device *rmi_dev)
 		return ret;
 	}
 
-	data->enabled = true;
-
 	return 0;
 }
 
@@ -886,23 +896,27 @@ void rmi_enable_irq(struct rmi_device *rmi_dev, bool clear_wake)
 	if (data->enabled)
 		goto out;
 
-	enable_irq(irq);
-	data->enabled = true;
-	if (clear_wake && device_may_wakeup(rmi_dev->xport->dev)) {
-		retval = disable_irq_wake(irq);
-		if (retval)
-			dev_warn(&rmi_dev->dev,
-				 "Failed to disable irq for wake: %d\n",
-				 retval);
-	}
+	if (irq) {
+		enable_irq(irq);
+		data->enabled = true;
+		if (clear_wake && device_may_wakeup(rmi_dev->xport->dev)) {
+			retval = disable_irq_wake(irq);
+			if (retval)
+				dev_warn(&rmi_dev->dev,
+					 "Failed to disable irq for wake: %d\n",
+					 retval);
+		}
 
-	/*
-	 * Call rmi_process_interrupt_requests() after enabling irq,
-	 * otherwise we may lose interrupt on edge-triggered systems.
-	 */
-	irq_flags = irq_get_trigger_type(pdata->irq);
-	if (irq_flags & IRQ_TYPE_EDGE_BOTH)
-		rmi_process_interrupt_requests(rmi_dev);
+		/*
+		 * Call rmi_process_interrupt_requests() after enabling irq,
+		 * otherwise we may lose interrupt on edge-triggered systems.
+		 */
+		irq_flags = irq_get_trigger_type(pdata->irq);
+		if (irq_flags & IRQ_TYPE_EDGE_BOTH)
+			rmi_process_interrupt_requests(rmi_dev);
+	} else {
+		data->enabled = true;
+	}
 
 out:
 	mutex_unlock(&data->enabled_mutex);
@@ -922,20 +936,22 @@ void rmi_disable_irq(struct rmi_device *rmi_dev, bool enable_wake)
 		goto out;
 
 	data->enabled = false;
-	disable_irq(irq);
-	if (enable_wake && device_may_wakeup(rmi_dev->xport->dev)) {
-		retval = enable_irq_wake(irq);
-		if (retval)
-			dev_warn(&rmi_dev->dev,
-				 "Failed to enable irq for wake: %d\n",
-				 retval);
-	}
-
-	/* make sure the fifo is clean */
-	while (!kfifo_is_empty(&data->attn_fifo)) {
-		count = kfifo_get(&data->attn_fifo, &attn_data);
-		if (count)
-			kfree(attn_data.data);
+	if (irq) {
+		disable_irq(irq);
+		if (enable_wake && device_may_wakeup(rmi_dev->xport->dev)) {
+			retval = enable_irq_wake(irq);
+			if (retval)
+				dev_warn(&rmi_dev->dev,
+					 "Failed to enable irq for wake: %d\n",
+					 retval);
+		}
+	} else {
+		/* make sure the fifo is clean */
+		while (!kfifo_is_empty(&data->attn_fifo)) {
+			count = kfifo_get(&data->attn_fifo, &attn_data);
+			if (count)
+				kfree(attn_data.data);
+		}
 	}
 
 out:
@@ -981,6 +997,8 @@ static int rmi_driver_remove(struct device *dev)
 	irq_domain_remove(data->irqdomain);
 	data->irqdomain = NULL;
 
+	cancel_work_sync(&data->attn_work);
+
 	rmi_f34_remove_sysfs(rmi_dev);
 	rmi_free_function_list(rmi_dev);
 
@@ -1219,9 +1237,15 @@ static int rmi_driver_probe(struct device *dev)
 		}
 	}
 
-	retval = rmi_irq_init(rmi_dev);
-	if (retval < 0)
-		goto err_destroy_functions;
+	if (pdata->irq) {
+		retval = rmi_irq_init(rmi_dev);
+		if (retval < 0)
+			goto err_destroy_functions;
+	}
+
+	data->enabled = true;
+
+	INIT_WORK(&data->attn_work, attn_callback);
 
 	if (data->f01_container->dev.driver) {
 		/* Driver already bound, so enable ATTN now. */
diff --git a/drivers/iommu/iommu.c b/drivers/iommu/iommu.c
index 3a67e636287a..eb5e796277d6 100644
--- a/drivers/iommu/iommu.c
+++ b/drivers/iommu/iommu.c
@@ -8,6 +8,7 @@
 
 #include <linux/amba/bus.h>
 #include <linux/device.h>
+#include <linux/dmi.h>
 #include <linux/kernel.h>
 #include <linux/bits.h>
 #include <linux/bug.h>
@@ -2931,6 +2932,27 @@ int iommu_dev_disable_feature(struct device *dev, enum iommu_dev_features feat)
 }
 EXPORT_SYMBOL_GPL(iommu_dev_disable_feature);
 
+#ifdef CONFIG_ARM64
+static int __init iommu_quirks(void)
+{
+	const char *vendor, *name;
+
+	vendor = dmi_get_system_info(DMI_SYS_VENDOR);
+	name = dmi_get_system_info(DMI_PRODUCT_NAME);
+
+	if (vendor &&
+	    (strncmp(vendor, "GIGABYTE", 8) == 0 && name &&
+	     (strncmp(name, "R120", 4) == 0 ||
+	      strncmp(name, "R270", 4) == 0))) {
+		pr_warn("Gigabyte %s detected, force iommu passthrough mode", name);
+		iommu_def_domain_type = IOMMU_DOMAIN_IDENTITY;
+	}
+
+	return 0;
+}
+arch_initcall(iommu_quirks);
+#endif
+
 /**
  * iommu_setup_default_domain - Set the default_domain for the group
  * @group: Group to change
diff --git a/drivers/pci/quirks.c b/drivers/pci/quirks.c
index b3976dcb71f1..54b122be6f35 100644
--- a/drivers/pci/quirks.c
+++ b/drivers/pci/quirks.c
@@ -4426,6 +4426,30 @@ DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_BROADCOM, 0x9000,
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_BROADCOM, 0x9084,
 				quirk_bridge_cavm_thrx2_pcie_root);
 
+/*
+ * PCI BAR 5 is not setup correctly for the on-board AHCI controller
+ * on Broadcom's Vulcan processor. Added a quirk to fix BAR 5 by
+ * using BAR 4's resources which are populated correctly and NOT
+ * actually used by the AHCI controller.
+ */
+static void quirk_fix_vulcan_ahci_bars(struct pci_dev *dev)
+{
+	struct resource *r =  &dev->resource[4];
+
+	if (!(r->flags & IORESOURCE_MEM) || (r->start == 0))
+		return;
+
+	/* Set BAR5 resource to BAR4 */
+	dev->resource[5] = *r;
+
+	/* Update BAR5 in pci config space */
+	pci_write_config_dword(dev, PCI_BASE_ADDRESS_5, r->start);
+
+	/* Clear BAR4's resource */
+	memset(r, 0, sizeof(*r));
+}
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_BROADCOM, 0x9027, quirk_fix_vulcan_ahci_bars);
+
 /*
  * Intersil/Techwell TW686[4589]-based video capture cards have an empty (zero)
  * class code.  Fix it.
diff --git a/drivers/scsi/sd.c b/drivers/scsi/sd.c
index e80c33cdad2b..3064ada8b6b8 100644
--- a/drivers/scsi/sd.c
+++ b/drivers/scsi/sd.c
@@ -118,6 +118,14 @@ static const char *sd_cache_types[] = {
 	"write back, no read (daft)"
 };
 
+static const char *sd_probe_types[] = { "async", "sync" };
+
+static char sd_probe_type[6] = "async";
+module_param_string(probe, sd_probe_type, sizeof(sd_probe_type),
+		    S_IRUGO|S_IWUSR);
+MODULE_PARM_DESC(probe, "async or sync. Setting to 'sync' disables asynchronous "
+		 "device number assignments (sda, sdb, ...).");
+
 static void sd_set_flush_flag(struct scsi_disk *sdkp)
 {
 	bool wc = false, fua = false;
@@ -4084,6 +4092,8 @@ static int __init init_sd(void)
 		goto err_out_class;
 	}
 
+	if (!strcmp(sd_probe_type, "sync"))
+		sd_template.gendrv.probe_type = PROBE_FORCE_SYNCHRONOUS;
 	err = scsi_register_driver(&sd_template.gendrv);
 	if (err)
 		goto err_out_driver;
diff --git a/include/linux/efi.h b/include/linux/efi.h
index 80b21d1c6eaf..b66c0683f2fc 100644
--- a/include/linux/efi.h
+++ b/include/linux/efi.h
@@ -44,6 +44,8 @@ struct screen_info;
 #define EFI_ABORTED		(21 | (1UL << (BITS_PER_LONG-1)))
 #define EFI_SECURITY_VIOLATION	(26 | (1UL << (BITS_PER_LONG-1)))
 
+#define EFI_IS_ERROR(x)		((x) & (1UL << (BITS_PER_LONG-1)))
+
 typedef unsigned long efi_status_t;
 typedef u8 efi_bool_t;
 typedef u16 efi_char16_t;		/* UNICODE character */
@@ -871,6 +873,14 @@ extern int __init efi_setup_pcdp_console(char *);
 #define EFI_MEM_ATTR		10	/* Did firmware publish an EFI_MEMORY_ATTRIBUTES table? */
 #define EFI_MEM_NO_SOFT_RESERVE	11	/* Is the kernel configured to ignore soft reservations? */
 #define EFI_PRESERVE_BS_REGIONS	12	/* Are EFI boot-services memory segments available? */
+#define EFI_SECURE_BOOT		13	/* Are we in Secure Boot mode? */
+
+enum efi_secureboot_mode {
+	efi_secureboot_mode_unset,
+	efi_secureboot_mode_unknown,
+	efi_secureboot_mode_disabled,
+	efi_secureboot_mode_enabled,
+};
 
 #ifdef CONFIG_EFI
 /*
@@ -882,6 +892,8 @@ static inline bool efi_enabled(int feature)
 }
 extern void efi_reboot(enum reboot_mode reboot_mode, const char *__unused);
 
+extern void __init efi_set_secure_boot(enum efi_secureboot_mode mode);
+
 bool __pure __efi_soft_reserve_enabled(void);
 
 static inline bool __pure efi_soft_reserve_enabled(void)
@@ -903,6 +915,8 @@ static inline bool efi_enabled(int feature)
 static inline void
 efi_reboot(enum reboot_mode reboot_mode, const char *__unused) {}
 
+static inline void efi_set_secure_boot(enum efi_secureboot_mode mode) {}
+
 static inline bool efi_soft_reserve_enabled(void)
 {
 	return false;
@@ -917,6 +931,7 @@ static inline void efi_find_mirror(void) {}
 #endif
 
 extern int efi_status_to_err(efi_status_t status);
+extern const char *efi_status_to_str(efi_status_t status);
 
 /*
  * Variable Attributes
@@ -1133,13 +1148,6 @@ static inline bool efi_runtime_disabled(void) { return true; }
 extern void efi_call_virt_check_flags(unsigned long flags, const void *caller);
 extern unsigned long efi_call_virt_save_flags(void);
 
-enum efi_secureboot_mode {
-	efi_secureboot_mode_unset,
-	efi_secureboot_mode_unknown,
-	efi_secureboot_mode_disabled,
-	efi_secureboot_mode_enabled,
-};
-
 static inline
 enum efi_secureboot_mode efi_get_secureboot_mode(efi_get_variable_t *get_var)
 {
diff --git a/include/linux/lsm_hook_defs.h b/include/linux/lsm_hook_defs.h
index 489362b0cd85..49933ea3afa9 100644
--- a/include/linux/lsm_hook_defs.h
+++ b/include/linux/lsm_hook_defs.h
@@ -407,6 +407,8 @@ LSM_HOOK(void, LSM_RET_VOID, bpf_prog_free_security, struct bpf_prog_aux *aux)
 #endif /* CONFIG_BPF_SYSCALL */
 
 LSM_HOOK(int, 0, locked_down, enum lockdown_reason what)
+LSM_HOOK(int, 0, lock_kernel_down, const char *where, enum lockdown_reason level)
+
 
 #ifdef CONFIG_PERF_EVENTS
 LSM_HOOK(int, 0, perf_event_open, struct perf_event_attr *attr, int type)
diff --git a/include/linux/module.h b/include/linux/module.h
index a98e188cf37b..2eef4246c2c9 100644
--- a/include/linux/module.h
+++ b/include/linux/module.h
@@ -418,6 +418,7 @@ struct module {
 	struct module_attribute *modinfo_attrs;
 	const char *version;
 	const char *srcversion;
+	const char *rhelversion;
 	struct kobject *holders_dir;
 
 	/* Exported symbols */
diff --git a/include/linux/rh_kabi.h b/include/linux/rh_kabi.h
new file mode 100644
index 000000000000..e0d3353802bb
--- /dev/null
+++ b/include/linux/rh_kabi.h
@@ -0,0 +1,172 @@
+/*
+ * rh_kabi.h - Red Hat kABI abstraction header
+ *
+ * Copyright (c) 2014 Don Zickus
+ * Copyright (c) 2015-2017 Jiri Benc
+ * Copyright (c) 2015 Sabrina Dubroca, Hannes Frederic Sowa
+ * Copyright (c) 2016-2018 Prarit Bhargava
+ * Copyright (c) 2017 Paolo Abeni, Larry Woodman
+ *
+ * This file is released under the GPLv2.
+ * See the file COPYING for more details.
+ *
+ * These kabi macros hide the changes from the kabi checker and from the
+ * process that computes the exported symbols' checksums.
+ * They have 2 variants: one (defined under __GENKSYMS__) used when
+ * generating the checksums, and the other used when building the kernel's
+ * binaries.
+ *
+ * The use of these macros does not guarantee that the usage and modification
+ * of code is correct.  As with all Red Hat only changes, an engineer must
+ * explain why the use of the macro is valid in the patch containing the
+ * changes.
+ *
+ */
+
+#ifndef _LINUX_RH_KABI_H
+#define _LINUX_RH_KABI_H
+
+#include <linux/compiler.h>
+#include <linux/stringify.h>
+
+/*
+ * RH_KABI_CONST
+ *   Adds a new const modifier to a function parameter preserving the old
+ *   checksum.
+ *
+ * RH_KABI_DEPRECATE
+ *   Mark the element as deprecated and make it unusable by modules while
+ *   preserving kABI checksums.
+ *
+ * RH_KABI_DEPRECATE_FN
+ *   Mark the function pointer as deprecated and make it unusable by modules
+ *   while preserving kABI checksums.
+ *
+ * RH_KABI_EXTEND
+ *   Simple macro for adding a new element to a struct.
+ *
+ *   Warning: only use if a hole exists for _all_ arches.  Use pahole to verify.
+ *
+ * RH_KABI_FILL_HOLE
+ *   Simple macro for filling a hole in a struct.
+ *
+ * RH_KABI_RENAME
+ *   Simple macro for renaming an element without changing its type.  This
+ *   macro can be used in bitfields, for example.
+ *
+ *   NOTE: does not include the final ';'
+ *
+ * RH_KABI_REPLACE
+ *   Simple replacement of _orig with a union of _orig and _new.
+ *
+ *   The RH_KABI_REPLACE* macros attempt to add the ability to use the '_new'
+ *   element while preserving size alignment with the '_orig' element.
+ *
+ *   The #ifdef __GENKSYMS__ preserves the kABI agreement, while the anonymous
+ *   union structure preserves the size alignment (assuming the '_new' element
+ *   is not bigger than the '_orig' element).
+ *
+ * RH_KABI_REPLACE_UNSAFE
+ *   Unsafe version of RH_KABI_REPLACE.  Only use for typedefs.
+ *
+ * RH_KABI_FORCE_CHANGE
+ *   Force change of the symbol checksum.  The argument of the macro is a
+ *   version for cases we need to do this more than once.
+ *
+ *   This macro does the opposite: it changes the symbol checksum without
+ *   actually changing anything about the exported symbol.  It is useful for
+ *   symbols that are not whitelisted, we're changing them in an
+ *   incompatible way and want to prevent 3rd party modules to silently
+ *   corrupt memory.  Instead, by changing the symbol checksum, such modules
+ *   won't be loaded by the kernel.  This macro should only be used as a
+ *   last resort when all other KABI workarounds have failed.
+ *
+ * NOTE
+ *   Don't use ';' after these macros as it messes up the kABI checker by
+ *   changing what the resulting token string looks like.  Instead let this
+ *   macro add the ';' so it can be properly hidden from the kABI checker
+ *   (mainly for RH_KABI_EXTEND, but applied to all macros for uniformity).
+ *
+ */
+#ifdef __GENKSYMS__
+
+# define RH_KABI_CONST
+# define RH_KABI_EXTEND(_new)
+# define RH_KABI_FILL_HOLE(_new)
+# define RH_KABI_FORCE_CHANGE(ver)		__attribute__((rh_kabi_change ## ver))
+# define RH_KABI_RENAME(_orig, _new)		_orig
+
+# define _RH_KABI_DEPRECATE(_type, _orig)	_type _orig
+# define _RH_KABI_DEPRECATE_FN(_type, _orig, _args...)	_type (*_orig)(_args)
+# define _RH_KABI_REPLACE(_orig, _new)		_orig
+# define _RH_KABI_REPLACE_UNSAFE(_orig, _new)	_orig
+
+#else
+
+# define RH_KABI_ALIGN_WARNING ".  Disable CONFIG_RH_KABI_SIZE_ALIGN_CHECKS if debugging."
+
+# define RH_KABI_CONST				const
+# define RH_KABI_EXTEND(_new)			_new;
+# define RH_KABI_FILL_HOLE(_new)		_new;
+# define RH_KABI_FORCE_CHANGE(ver)
+# define RH_KABI_RENAME(_orig, _new)		_new
+
+
+#if IS_BUILTIN(CONFIG_RH_KABI_SIZE_ALIGN_CHECKS)
+# define __RH_KABI_CHECK_SIZE_ALIGN(_orig, _new)			\
+	union {								\
+		_Static_assert(sizeof(struct{_new;}) <= sizeof(struct{_orig;}), \
+			       __FILE__ ":" __stringify(__LINE__) ": "  __stringify(_new) " is larger than " __stringify(_orig) RH_KABI_ALIGN_WARNING); \
+		_Static_assert(__alignof__(struct{_new;}) <= __alignof__(struct{_orig;}), \
+			       __FILE__ ":" __stringify(__LINE__) ": "  __stringify(_orig) " is not aligned the same as " __stringify(_new) RH_KABI_ALIGN_WARNING); \
+	}
+#else
+# define __RH_KABI_CHECK_SIZE_ALIGN(_orig, _new)
+#endif
+
+# define _RH_KABI_DEPRECATE(_type, _orig)	_type rh_reserved_##_orig
+# define _RH_KABI_DEPRECATE_FN(_type, _orig, _args...)  \
+	_type (* rh_reserved_##_orig)(_args)
+# define _RH_KABI_REPLACE(_orig, _new)			  \
+	union {						  \
+		_new;					  \
+		struct {				  \
+			_orig;				  \
+		} __UNIQUE_ID(rh_kabi_hide);		  \
+		__RH_KABI_CHECK_SIZE_ALIGN(_orig, _new);  \
+	}
+# define _RH_KABI_REPLACE_UNSAFE(_orig, _new)	_new
+
+#endif /* __GENKSYMS__ */
+
+/* semicolon added wrappers for the RH_KABI_REPLACE macros */
+# define RH_KABI_DEPRECATE(_type, _orig)	_RH_KABI_DEPRECATE(_type, _orig);
+# define RH_KABI_DEPRECATE_FN(_type, _orig, _args...)  \
+	_RH_KABI_DEPRECATE_FN(_type, _orig, _args);
+# define RH_KABI_REPLACE(_orig, _new)		_RH_KABI_REPLACE(_orig, _new);
+# define RH_KABI_REPLACE_UNSAFE(_orig, _new)	_RH_KABI_REPLACE_UNSAFE(_orig, _new);
+/*
+ * Macro for breaking up a random element into two smaller chunks using an
+ * anonymous struct inside an anonymous union.
+ */
+# define RH_KABI_REPLACE2(orig, _new1, _new2)	RH_KABI_REPLACE(orig, struct{ _new1; _new2;})
+
+# define RH_KABI_RESERVE(n)		_RH_KABI_RESERVE(n);
+/*
+ * Simple wrappers to replace standard Red Hat reserved elements.
+ */
+# define RH_KABI_USE(n, _new)		RH_KABI_REPLACE(_RH_KABI_RESERVE(n), _new)
+/*
+ * Macros for breaking up a reserved element into two smaller chunks using
+ * an anonymous struct inside an anonymous union.
+ */
+# define RH_KABI_USE2(n, _new1, _new2)	RH_KABI_REPLACE(_RH_KABI_RESERVE(n), struct{ _new1; _new2; })
+
+/*
+ * We tried to standardize on Red Hat reserved names.  These wrappers
+ * leverage those common names making it easier to read and find in the
+ * code.
+ */
+# define _RH_KABI_RESERVE(n)		unsigned long rh_reserved##n
+
+#endif /* _LINUX_RH_KABI_H */
diff --git a/include/linux/rmi.h b/include/linux/rmi.h
index ab7eea01ab42..fff7c5f737fc 100644
--- a/include/linux/rmi.h
+++ b/include/linux/rmi.h
@@ -364,6 +364,7 @@ struct rmi_driver_data {
 
 	struct rmi4_attn_data attn_data;
 	DECLARE_KFIFO(attn_fifo, struct rmi4_attn_data, 16);
+	struct work_struct attn_work;
 };
 
 int rmi_register_transport_device(struct rmi_transport_dev *xport);
diff --git a/include/linux/security.h b/include/linux/security.h
index b50c7f566189..8a12e0f0a0fe 100644
--- a/include/linux/security.h
+++ b/include/linux/security.h
@@ -486,6 +486,7 @@ int security_inode_notifysecctx(struct inode *inode, void *ctx, u32 ctxlen);
 int security_inode_setsecctx(struct dentry *dentry, void *ctx, u32 ctxlen);
 int security_inode_getsecctx(struct inode *inode, void **ctx, u32 *ctxlen);
 int security_locked_down(enum lockdown_reason what);
+int security_lock_kernel_down(const char *where, enum lockdown_reason level);
 #else /* CONFIG_SECURITY */
 
 static inline int call_blocking_lsm_notifier(enum lsm_event event, void *data)
@@ -1404,6 +1405,10 @@ static inline int security_locked_down(enum lockdown_reason what)
 {
 	return 0;
 }
+static inline int security_lock_kernel_down(const char *where, enum lockdown_reason level)
+{
+	return 0;
+}
 #endif	/* CONFIG_SECURITY */
 
 #if defined(CONFIG_SECURITY) && defined(CONFIG_WATCH_QUEUE)
diff --git a/kernel/module/main.c b/kernel/module/main.c
index 34d9e718c2c7..1c8b40b19014 100644
--- a/kernel/module/main.c
+++ b/kernel/module/main.c
@@ -528,6 +528,7 @@ static struct module_attribute modinfo_##field = {                    \
 
 MODINFO_ATTR(version);
 MODINFO_ATTR(srcversion);
+MODINFO_ATTR(rhelversion);
 
 static struct {
 	char name[MODULE_NAME_LEN + 1];
@@ -980,6 +981,7 @@ struct module_attribute *modinfo_attrs[] = {
 	&module_uevent,
 	&modinfo_version,
 	&modinfo_srcversion,
+	&modinfo_rhelversion,
 	&modinfo_initstate,
 	&modinfo_coresize,
 #ifdef CONFIG_ARCH_WANTS_MODULES_DATA_IN_VMALLOC
diff --git a/kernel/module/signing.c b/kernel/module/signing.c
index a2ff4242e623..f0d2be1ee4f1 100644
--- a/kernel/module/signing.c
+++ b/kernel/module/signing.c
@@ -61,10 +61,17 @@ int mod_verify_sig(const void *mod, struct load_info *info)
 	modlen -= sig_len + sizeof(ms);
 	info->len = modlen;
 
-	return verify_pkcs7_signature(mod, modlen, mod + modlen, sig_len,
+	ret = verify_pkcs7_signature(mod, modlen, mod + modlen, sig_len,
 				      VERIFY_USE_SECONDARY_KEYRING,
 				      VERIFYING_MODULE_SIGNATURE,
 				      NULL, NULL);
+	if (ret == -ENOKEY && IS_ENABLED(CONFIG_INTEGRITY_PLATFORM_KEYRING)) {
+		ret = verify_pkcs7_signature(mod, modlen, mod + modlen, sig_len,
+				VERIFY_USE_PLATFORM_KEYRING,
+				VERIFYING_MODULE_SIGNATURE,
+				NULL, NULL);
+	}
+	return ret;
 }
 
 int module_sig_check(struct load_info *info, int flags)
diff --git a/scripts/tags.sh b/scripts/tags.sh
index a70d43723146..56d06b04f752 100755
--- a/scripts/tags.sh
+++ b/scripts/tags.sh
@@ -16,6 +16,8 @@ fi
 ignore="$(echo "$RCS_FIND_IGNORE" | sed 's|\\||g' )"
 # tags and cscope files should also ignore MODVERSION *.mod.c files
 ignore="$ignore ( -name *.mod.c ) -prune -o"
+# RHEL tags and cscope should also ignore redhat/rpm
+ignore="$ignore ( -path redhat/rpm ) -prune -o"
 
 # ignore arbitrary directories
 if [ -n "${IGNORE_DIRS}" ]; then
diff --git a/security/integrity/platform_certs/load_uefi.c b/security/integrity/platform_certs/load_uefi.c
index d1fdd113450a..182e8090cfe8 100644
--- a/security/integrity/platform_certs/load_uefi.c
+++ b/security/integrity/platform_certs/load_uefi.c
@@ -74,7 +74,8 @@ static __init void *get_cert_list(efi_char16_t *name, efi_guid_t *guid,
 		return NULL;
 
 	if (*status != EFI_BUFFER_TOO_SMALL) {
-		pr_err("Couldn't get size: 0x%lx\n", *status);
+		pr_err("Couldn't get size: %s (0x%lx)\n",
+		       efi_status_to_str(*status), *status);
 		return NULL;
 	}
 
@@ -85,7 +86,8 @@ static __init void *get_cert_list(efi_char16_t *name, efi_guid_t *guid,
 	*status = efi.get_variable(name, guid, NULL, &lsize, db);
 	if (*status != EFI_SUCCESS) {
 		kfree(db);
-		pr_err("Error reading db var: 0x%lx\n", *status);
+		pr_err("Error reading db var: %s (0x%lx)\n",
+		       efi_status_to_str(*status), *status);
 		return NULL;
 	}
 
diff --git a/security/lockdown/Kconfig b/security/lockdown/Kconfig
index e84ddf484010..d0501353a4b9 100644
--- a/security/lockdown/Kconfig
+++ b/security/lockdown/Kconfig
@@ -16,6 +16,19 @@ config SECURITY_LOCKDOWN_LSM_EARLY
 	  subsystem is fully initialised. If enabled, lockdown will
 	  unconditionally be called before any other LSMs.
 
+config LOCK_DOWN_IN_EFI_SECURE_BOOT
+	bool "Lock down the kernel in EFI Secure Boot mode"
+	default n
+	depends on EFI && SECURITY_LOCKDOWN_LSM_EARLY
+	help
+	  UEFI Secure Boot provides a mechanism for ensuring that the firmware
+	  will only load signed bootloaders and kernels.  Secure boot mode may
+	  be determined from EFI variables provided by the system firmware if
+	  not indicated by the boot parameters.
+
+	  Enabling this option results in kernel lockdown being triggered if
+	  EFI Secure Boot is set.
+
 choice
 	prompt "Kernel default lockdown mode"
 	default LOCK_DOWN_KERNEL_FORCE_NONE
diff --git a/security/lockdown/lockdown.c b/security/lockdown/lockdown.c
index 68d19632aeb7..ef348935b6ff 100644
--- a/security/lockdown/lockdown.c
+++ b/security/lockdown/lockdown.c
@@ -73,6 +73,7 @@ static int lockdown_is_locked_down(enum lockdown_reason what)
 
 static struct security_hook_list lockdown_hooks[] __ro_after_init = {
 	LSM_HOOK_INIT(locked_down, lockdown_is_locked_down),
+	LSM_HOOK_INIT(lock_kernel_down, lock_kernel_down),
 };
 
 static int __init lockdown_lsm_init(void)
diff --git a/security/security.c b/security/security.c
index 407b51719f79..bffb48f02087 100644
--- a/security/security.c
+++ b/security/security.c
@@ -5283,6 +5283,18 @@ int security_locked_down(enum lockdown_reason what)
 }
 EXPORT_SYMBOL(security_locked_down);
 
+/**
+ * security_lock_kernel_down() - Put the kernel into lock-down mode.
+ *
+ * @where: Where the lock-down is originating from (e.g. command line option)
+ * @level: The lock-down level (can only increase)
+ */
+int security_lock_kernel_down(const char *where, enum lockdown_reason level)
+{
+	return call_int_hook(lock_kernel_down, 0, where, level);
+}
+EXPORT_SYMBOL(security_lock_kernel_down);
+
 #ifdef CONFIG_PERF_EVENTS
 /**
  * security_perf_event_open() - Check if a perf event open is allowed
diff --git a/sound/pci/hda/cs35l41_hda.c b/sound/pci/hda/cs35l41_hda.c
index 3c157b006a5a..257f71e9ec07 100644
--- a/sound/pci/hda/cs35l41_hda.c
+++ b/sound/pci/hda/cs35l41_hda.c
@@ -33,6 +33,9 @@
 #define CAL_AMBIENT_DSP_CTL_NAME	"CAL_AMBIENT"
 #define CAL_DSP_CTL_TYPE		5
 #define CAL_DSP_CTL_ALG			205
+#define CS35L41_UUID			"50d90cdc-3de4-4f18-b528-c7fe3b71f40d"
+#define CS35L41_DSM_GET_MUTE		5
+#define CS35L41_NOTIFY_EVENT		0x91
 
 static bool firmware_autostart = 1;
 module_param(firmware_autostart, bool, 0444);
@@ -563,6 +566,31 @@ static void cs35l41_hda_play_start(struct device *dev)
 
 }
 
+static void cs35l41_mute(struct device *dev, bool mute)
+{
+	struct cs35l41_hda *cs35l41 = dev_get_drvdata(dev);
+	struct regmap *reg = cs35l41->regmap;
+
+	dev_dbg(dev, "Mute(%d:%d) Playback Started: %d\n", mute, cs35l41->mute_override,
+		cs35l41->playback_started);
+
+	if (cs35l41->playback_started) {
+		if (mute || cs35l41->mute_override) {
+			dev_dbg(dev, "Muting\n");
+			regmap_multi_reg_write(reg, cs35l41_hda_mute, ARRAY_SIZE(cs35l41_hda_mute));
+		} else {
+			dev_dbg(dev, "Unmuting\n");
+			if (cs35l41->firmware_running) {
+				regmap_multi_reg_write(reg, cs35l41_hda_unmute_dsp,
+						ARRAY_SIZE(cs35l41_hda_unmute_dsp));
+			} else {
+				regmap_multi_reg_write(reg, cs35l41_hda_unmute,
+						ARRAY_SIZE(cs35l41_hda_unmute));
+			}
+		}
+	}
+}
+
 static void cs35l41_hda_play_done(struct device *dev)
 {
 	struct cs35l41_hda *cs35l41 = dev_get_drvdata(dev);
@@ -572,13 +600,7 @@ static void cs35l41_hda_play_done(struct device *dev)
 
 	cs35l41_global_enable(dev, reg, cs35l41->hw_cfg.bst_type, 1,
 			      cs35l41->firmware_running);
-	if (cs35l41->firmware_running) {
-		regmap_multi_reg_write(reg, cs35l41_hda_unmute_dsp,
-				       ARRAY_SIZE(cs35l41_hda_unmute_dsp));
-	} else {
-		regmap_multi_reg_write(reg, cs35l41_hda_unmute,
-				       ARRAY_SIZE(cs35l41_hda_unmute));
-	}
+	cs35l41_mute(dev, false);
 }
 
 static void cs35l41_hda_pause_start(struct device *dev)
@@ -588,7 +610,7 @@ static void cs35l41_hda_pause_start(struct device *dev)
 
 	dev_dbg(dev, "Pause (Start)\n");
 
-	regmap_multi_reg_write(reg, cs35l41_hda_mute, ARRAY_SIZE(cs35l41_hda_mute));
+	cs35l41_mute(dev, true);
 	cs35l41_global_enable(dev, reg, cs35l41->hw_cfg.bst_type, 0,
 			      cs35l41->firmware_running);
 }
@@ -1116,6 +1138,53 @@ static int cs35l41_create_controls(struct cs35l41_hda *cs35l41)
 	return 0;
 }
 
+static bool cs35l41_dsm_supported(acpi_handle handle, unsigned int commands)
+{
+	guid_t guid;
+
+	guid_parse(CS35L41_UUID, &guid);
+
+	return acpi_check_dsm(handle, &guid, 0, BIT(commands));
+}
+
+static int cs35l41_get_acpi_mute_state(struct cs35l41_hda *cs35l41, acpi_handle handle)
+{
+	guid_t guid;
+	union acpi_object *ret;
+	int mute = -ENODEV;
+
+	guid_parse(CS35L41_UUID, &guid);
+
+	if (cs35l41_dsm_supported(handle, CS35L41_DSM_GET_MUTE)) {
+		ret = acpi_evaluate_dsm(handle, &guid, 0, CS35L41_DSM_GET_MUTE, NULL);
+		mute = *ret->buffer.pointer;
+		dev_dbg(cs35l41->dev, "CS35L41_DSM_GET_MUTE: %d\n", mute);
+	}
+
+	dev_dbg(cs35l41->dev, "%s: %d\n", __func__, mute);
+
+	return mute;
+}
+
+static void cs35l41_acpi_device_notify(acpi_handle handle, u32 event, struct device *dev)
+{
+	struct cs35l41_hda *cs35l41 = dev_get_drvdata(dev);
+	int mute;
+
+	if (event != CS35L41_NOTIFY_EVENT)
+		return;
+
+	mute = cs35l41_get_acpi_mute_state(cs35l41, handle);
+	if (mute < 0) {
+		dev_warn(cs35l41->dev, "Unable to retrieve mute state: %d\n", mute);
+		return;
+	}
+
+	dev_dbg(cs35l41->dev, "Requesting mute value: %d\n", mute);
+	cs35l41->mute_override = (mute > 0);
+	cs35l41_mute(cs35l41->dev, cs35l41->mute_override);
+}
+
 static int cs35l41_hda_bind(struct device *dev, struct device *master, void *master_data)
 {
 	struct cs35l41_hda *cs35l41 = dev_get_drvdata(dev);
@@ -1157,6 +1226,14 @@ static int cs35l41_hda_bind(struct device *dev, struct device *master, void *mas
 	comps->playback_hook = cs35l41_hda_playback_hook;
 	comps->pre_playback_hook = cs35l41_hda_pre_playback_hook;
 	comps->post_playback_hook = cs35l41_hda_post_playback_hook;
+	comps->acpi_notify = cs35l41_acpi_device_notify;
+	comps->adev = cs35l41->dacpi;
+
+	comps->acpi_notifications_supported = cs35l41_dsm_supported(acpi_device_handle(comps->adev),
+		CS35L41_DSM_GET_MUTE);
+
+	cs35l41->mute_override = cs35l41_get_acpi_mute_state(cs35l41,
+						acpi_device_handle(cs35l41->dacpi)) > 0;
 
 	mutex_unlock(&cs35l41->fw_mutex);
 
@@ -1430,8 +1507,8 @@ static int cs35l41_hda_read_acpi(struct cs35l41_hda *cs35l41, const char *hid, i
 		return -ENODEV;
 	}
 
+	cs35l41->dacpi = adev;
 	physdev = get_device(acpi_get_first_physical_node(adev));
-	acpi_dev_put(adev);
 
 	sub = acpi_get_subsystem_id(ACPI_HANDLE(physdev));
 	if (IS_ERR(sub))
@@ -1541,6 +1618,7 @@ static int cs35l41_hda_read_acpi(struct cs35l41_hda *cs35l41, const char *hid, i
 	hw_cfg->valid = false;
 	hw_cfg->gpio1.valid = false;
 	hw_cfg->gpio2.valid = false;
+	acpi_dev_put(cs35l41->dacpi);
 put_physdev:
 	put_device(physdev);
 
@@ -1644,10 +1722,7 @@ int cs35l41_hda_probe(struct device *dev, const char *device_name, int id, int i
 	if (ret)
 		goto err;
 
-	ret = regmap_multi_reg_write(cs35l41->regmap, cs35l41_hda_mute,
-				     ARRAY_SIZE(cs35l41_hda_mute));
-	if (ret)
-		goto err;
+	cs35l41_mute(cs35l41->dev, true);
 
 	INIT_WORK(&cs35l41->fw_load_work, cs35l41_fw_load_work);
 	mutex_init(&cs35l41->fw_mutex);
@@ -1684,6 +1759,8 @@ int cs35l41_hda_probe(struct device *dev, const char *device_name, int id, int i
 	if (cs35l41_safe_reset(cs35l41->regmap, cs35l41->hw_cfg.bst_type))
 		gpiod_set_value_cansleep(cs35l41->reset_gpio, 0);
 	gpiod_put(cs35l41->reset_gpio);
+	gpiod_put(cs35l41->cs_gpio);
+	acpi_dev_put(cs35l41->dacpi);
 	kfree(cs35l41->acpi_subsystem_id);
 
 	return ret;
@@ -1703,11 +1780,14 @@ void cs35l41_hda_remove(struct device *dev)
 
 	component_del(cs35l41->dev, &cs35l41_hda_comp_ops);
 
+	acpi_dev_put(cs35l41->dacpi);
+
 	pm_runtime_put_noidle(cs35l41->dev);
 
 	if (cs35l41_safe_reset(cs35l41->regmap, cs35l41->hw_cfg.bst_type))
 		gpiod_set_value_cansleep(cs35l41->reset_gpio, 0);
 	gpiod_put(cs35l41->reset_gpio);
+	gpiod_put(cs35l41->cs_gpio);
 	kfree(cs35l41->acpi_subsystem_id);
 }
 EXPORT_SYMBOL_NS_GPL(cs35l41_hda_remove, SND_HDA_SCODEC_CS35L41);
diff --git a/sound/pci/hda/cs35l41_hda.h b/sound/pci/hda/cs35l41_hda.h
index b93bf762976e..3d925d677213 100644
--- a/sound/pci/hda/cs35l41_hda.h
+++ b/sound/pci/hda/cs35l41_hda.h
@@ -10,6 +10,7 @@
 #ifndef __CS35L41_HDA_H__
 #define __CS35L41_HDA_H__
 
+#include <linux/acpi.h>
 #include <linux/efi.h>
 #include <linux/regulator/consumer.h>
 #include <linux/gpio/consumer.h>
@@ -34,8 +35,8 @@ struct cs35l41_amp_efi_data {
 } __packed;
 
 enum cs35l41_hda_spk_pos {
-	CS35l41_LEFT,
-	CS35l41_RIGHT,
+	CS35L41_LEFT,
+	CS35L41_RIGHT,
 };
 
 enum cs35l41_hda_gpio_function {
@@ -49,6 +50,7 @@ struct cs35l41_hda {
 	struct device *dev;
 	struct regmap *regmap;
 	struct gpio_desc *reset_gpio;
+	struct gpio_desc *cs_gpio;
 	struct cs35l41_hw_cfg hw_cfg;
 	struct hda_codec *codec;
 
@@ -70,6 +72,8 @@ struct cs35l41_hda {
 	bool halo_initialized;
 	bool playback_started;
 	struct cs_dsp cs_dsp;
+	struct acpi_device *dacpi;
+	bool mute_override;
 };
 
 enum halo_state {
diff --git a/sound/pci/hda/cs35l41_hda_property.c b/sound/pci/hda/cs35l41_hda_property.c
index b62a4e6968e2..c9eb70290973 100644
--- a/sound/pci/hda/cs35l41_hda_property.c
+++ b/sound/pci/hda/cs35l41_hda_property.c
@@ -6,9 +6,300 @@
 //
 // Author: Stefan Binding <sbinding@opensource.cirrus.com>
 
+#include <linux/acpi.h>
 #include <linux/gpio/consumer.h>
 #include <linux/string.h>
 #include "cs35l41_hda_property.h"
+#include <linux/spi/spi.h>
+
+#define MAX_AMPS 4
+
+struct cs35l41_config {
+	const char *ssid;
+	enum {
+		SPI,
+		I2C
+	} bus;
+	int num_amps;
+	enum {
+		INTERNAL,
+		EXTERNAL
+	} boost_type;
+	u8 channel[MAX_AMPS];
+	int reset_gpio_index; /* -1 if no reset gpio */
+	int spkid_gpio_index; /* -1 if no spkid gpio */
+	int cs_gpio_index; /* -1 if no cs gpio, or cs-gpios already exists, max num amps == 2 */
+	int boost_ind_nanohenry; /* Required if boost_type == Internal */
+	int boost_peak_milliamp; /* Required if boost_type == Internal */
+	int boost_cap_microfarad; /* Required if boost_type == Internal */
+};
+
+static const struct cs35l41_config cs35l41_config_table[] = {
+/*
+ * Device 103C89C6 does have _DSD, however it is setup to use the wrong boost type.
+ * We can override the _DSD to correct the boost type here.
+ * Since this laptop has valid ACPI, we do not need to handle cs-gpios, since that already exists
+ * in the ACPI. The Reset GPIO is also valid, so we can use the Reset defined in _DSD.
+ */
+	{ "103C89C6", SPI, 2, INTERNAL, { CS35L41_RIGHT, CS35L41_LEFT, 0, 0 }, -1, -1, -1, 1000, 4500, 24 },
+	{ "104312AF", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431433", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431463", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431473", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, -1, 0, 1000, 4500, 24 },
+	{ "10431483", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, -1, 0, 1000, 4500, 24 },
+	{ "10431493", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "104314D3", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "104314E3", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431503", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431533", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431573", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431663", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, -1, 0, 1000, 4500, 24 },
+	{ "104316D3", SPI, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 0, 0, 0 },
+	{ "104316F3", SPI, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 0, 0, 0 },
+	{ "104317F3", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431863", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "104318D3", I2C, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 0, 0, 0 },
+	{ "10431C9F", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431CAF", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431CCF", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431CDF", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431CEF", SPI, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 1000, 4500, 24 },
+	{ "10431D1F", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431DA2", SPI, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 0, 0, 0 },
+	{ "10431E02", SPI, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 0, 0, 0 },
+	{ "10431EE2", I2C, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, -1, -1, 0, 0, 0 },
+	{ "10431F12", I2C, 2, INTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 0, 1, -1, 1000, 4500, 24 },
+	{ "10431F1F", SPI, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, -1, 0, 0, 0, 0 },
+	{ "10431F62", SPI, 2, EXTERNAL, { CS35L41_LEFT, CS35L41_RIGHT, 0, 0 }, 1, 2, 0, 0, 0, 0 },
+	{}
+};
+
+static int cs35l41_add_gpios(struct cs35l41_hda *cs35l41, struct device *physdev, int reset_gpio,
+			     int spkid_gpio, int cs_gpio_index, int num_amps)
+{
+	struct acpi_gpio_mapping *gpio_mapping;
+	struct acpi_gpio_params *reset_gpio_params;
+	struct acpi_gpio_params *spkid_gpio_params;
+	struct acpi_gpio_params *cs_gpio_params;
+	unsigned int num_entries = 0;
+	unsigned int reset_index, spkid_index, csgpio_index;
+	int i;
+
+	/*
+	 * GPIO Mapping only needs to be done once, since it would be available for subsequent amps
+	 */
+	if (cs35l41->dacpi->driver_gpios)
+		return 0;
+
+	if (reset_gpio >= 0) {
+		reset_index = num_entries;
+		num_entries++;
+	}
+
+	if (spkid_gpio >= 0) {
+		spkid_index = num_entries;
+		num_entries++;
+	}
+
+	if ((cs_gpio_index >= 0)  && (num_amps == 2)) {
+		csgpio_index = num_entries;
+		num_entries++;
+	}
+
+	if (!num_entries)
+		return 0;
+
+	/* must include termination entry */
+	num_entries++;
+
+	gpio_mapping = devm_kcalloc(physdev, num_entries, sizeof(struct acpi_gpio_mapping),
+				    GFP_KERNEL);
+
+	if (!gpio_mapping)
+		goto err;
+
+	if (reset_gpio >= 0) {
+		gpio_mapping[reset_index].name = "reset-gpios";
+		reset_gpio_params = devm_kcalloc(physdev, num_amps, sizeof(struct acpi_gpio_params),
+						 GFP_KERNEL);
+		if (!reset_gpio_params)
+			goto err;
+
+		for (i = 0; i < num_amps; i++)
+			reset_gpio_params[i].crs_entry_index = reset_gpio;
+
+		gpio_mapping[reset_index].data = reset_gpio_params;
+		gpio_mapping[reset_index].size = num_amps;
+	}
+
+	if (spkid_gpio >= 0) {
+		gpio_mapping[spkid_index].name = "spk-id-gpios";
+		spkid_gpio_params = devm_kcalloc(physdev, num_amps, sizeof(struct acpi_gpio_params),
+						 GFP_KERNEL);
+		if (!spkid_gpio_params)
+			goto err;
+
+		for (i = 0; i < num_amps; i++)
+			spkid_gpio_params[i].crs_entry_index = spkid_gpio;
+
+		gpio_mapping[spkid_index].data = spkid_gpio_params;
+		gpio_mapping[spkid_index].size = num_amps;
+	}
+
+	if ((cs_gpio_index >= 0) && (num_amps == 2)) {
+		gpio_mapping[csgpio_index].name = "cs-gpios";
+		/* only one GPIO CS is supported without using _DSD, obtained using index 0 */
+		cs_gpio_params = devm_kzalloc(physdev, sizeof(struct acpi_gpio_params), GFP_KERNEL);
+		if (!cs_gpio_params)
+			goto err;
+
+		cs_gpio_params->crs_entry_index = cs_gpio_index;
+
+		gpio_mapping[csgpio_index].data = cs_gpio_params;
+		gpio_mapping[csgpio_index].size = 1;
+	}
+
+	return devm_acpi_dev_add_driver_gpios(physdev, gpio_mapping);
+err:
+	devm_kfree(physdev, gpio_mapping);
+	devm_kfree(physdev, reset_gpio_params);
+	devm_kfree(physdev, spkid_gpio_params);
+	devm_kfree(physdev, cs_gpio_params);
+	return -ENOMEM;
+}
+
+static int generic_dsd_config(struct cs35l41_hda *cs35l41, struct device *physdev, int id,
+			      const char *hid)
+{
+	struct cs35l41_hw_cfg *hw_cfg = &cs35l41->hw_cfg;
+	const struct cs35l41_config *cfg;
+	struct gpio_desc *cs_gpiod;
+	struct spi_device *spi;
+	bool dsd_found;
+	int ret;
+
+	for (cfg = cs35l41_config_table; cfg->ssid; cfg++) {
+		if (!strcasecmp(cfg->ssid, cs35l41->acpi_subsystem_id))
+			break;
+	}
+
+	if (!cfg->ssid)
+		return -ENOENT;
+
+	if (!cs35l41->dacpi || cs35l41->dacpi != ACPI_COMPANION(physdev)) {
+		dev_err(cs35l41->dev, "ACPI Device does not match, cannot override _DSD.\n");
+		return -ENODEV;
+	}
+
+	dev_info(cs35l41->dev, "Adding DSD properties for %s\n", cs35l41->acpi_subsystem_id);
+
+	dsd_found = acpi_dev_has_props(cs35l41->dacpi);
+
+	if (!dsd_found) {
+		ret = cs35l41_add_gpios(cs35l41, physdev, cfg->reset_gpio_index,
+						 cfg->spkid_gpio_index, cfg->cs_gpio_index,
+						 cfg->num_amps);
+		if (ret) {
+			dev_err(cs35l41->dev, "Error adding GPIO mapping: %d\n", ret);
+			return ret;
+		}
+	} else if (cfg->reset_gpio_index >= 0 || cfg->spkid_gpio_index >= 0) {
+		dev_warn(cs35l41->dev, "Cannot add Reset/Speaker ID/SPI CS GPIO Mapping, "
+			 "_DSD already exists.\n");
+	}
+
+	if (cfg->bus == SPI) {
+		cs35l41->index = id;
+		/*
+		 * Manually set the Chip Select for the second amp <cs_gpio_index> in the node.
+		 * This is only supported for systems with 2 amps, since we cannot expand the
+		 * default number of chip selects without using cs-gpios
+		 * The CS GPIO must be set high prior to communicating with the first amp (which
+		 * uses a native chip select), to ensure the second amp does not clash with the
+		 * first.
+		 */
+		if (cfg->cs_gpio_index >= 0) {
+			spi = to_spi_device(cs35l41->dev);
+
+			if (cfg->num_amps != 2) {
+				dev_warn(cs35l41->dev,
+					 "Cannot update SPI CS, Number of Amps (%d) != 2\n",
+					 cfg->num_amps);
+			} else if (dsd_found) {
+				dev_warn(cs35l41->dev,
+					"Cannot update SPI CS, _DSD already exists.\n");
+			} else {
+				/*
+				 * This is obtained using driver_gpios, since only one GPIO for CS
+				 * exists, this can be obtained using index 0.
+				 */
+				cs_gpiod = gpiod_get_index(physdev, "cs", 0, GPIOD_OUT_LOW);
+				if (IS_ERR(cs_gpiod)) {
+					dev_err(cs35l41->dev,
+						"Unable to get Chip Select GPIO descriptor\n");
+					return PTR_ERR(cs_gpiod);
+				}
+				if (id == 1) {
+					spi_set_csgpiod(spi, 0, cs_gpiod);
+					cs35l41->cs_gpio = cs_gpiod;
+				} else {
+					gpiod_set_value_cansleep(cs_gpiod, true);
+					gpiod_put(cs_gpiod);
+				}
+				spi_setup(spi);
+			}
+		}
+	} else {
+		if (cfg->num_amps > 2)
+			/*
+			 * i2c addresses for 3/4 amps are used in order: 0x40, 0x41, 0x42, 0x43,
+			 * subtracting 0x40 would give zero-based index
+			 */
+			cs35l41->index = id - 0x40;
+		else
+			/* i2c addr 0x40 for first amp (always), 0x41/0x42 for 2nd amp */
+			cs35l41->index = id == 0x40 ? 0 : 1;
+	}
+
+	if (cfg->num_amps == 3)
+		/* 3 amps means a center channel, so no duplicate channels */
+		cs35l41->channel_index = 0;
+	else
+		/*
+		 * if 4 amps, there are duplicate channels, so they need different indexes
+		 * if 2 amps, no duplicate channels, channel_index would be 0
+		 */
+		cs35l41->channel_index = cs35l41->index / 2;
+
+	cs35l41->reset_gpio = fwnode_gpiod_get_index(acpi_fwnode_handle(cs35l41->dacpi), "reset",
+						     cs35l41->index, GPIOD_OUT_LOW,
+						     "cs35l41-reset");
+	cs35l41->speaker_id = cs35l41_get_speaker_id(physdev, cs35l41->index, cfg->num_amps, -1);
+
+	hw_cfg->spk_pos = cfg->channel[cs35l41->index];
+
+	if (cfg->boost_type == INTERNAL) {
+		hw_cfg->bst_type = CS35L41_INT_BOOST;
+		hw_cfg->bst_ind = cfg->boost_ind_nanohenry;
+		hw_cfg->bst_ipk = cfg->boost_peak_milliamp;
+		hw_cfg->bst_cap = cfg->boost_cap_microfarad;
+		hw_cfg->gpio1.func = CS35L41_NOT_USED;
+		hw_cfg->gpio1.valid = true;
+	} else {
+		hw_cfg->bst_type = CS35L41_EXT_BOOST;
+		hw_cfg->bst_ind = -1;
+		hw_cfg->bst_ipk = -1;
+		hw_cfg->bst_cap = -1;
+		hw_cfg->gpio1.func = CS35l41_VSPK_SWITCH;
+		hw_cfg->gpio1.valid = true;
+	}
+
+	hw_cfg->gpio2.func = CS35L41_INTERRUPT;
+	hw_cfg->gpio2.valid = true;
+	hw_cfg->valid = true;
+
+	return 0;
+}
 
 /*
  * Device CLSA010(0/1) doesn't have _DSD so a gpiod_get by the label reset won't work.
@@ -43,37 +334,6 @@ static int lenovo_legion_no_acpi(struct cs35l41_hda *cs35l41, struct device *phy
 	return 0;
 }
 
-/*
- * Device 103C89C6 does have _DSD, however it is setup to use the wrong boost type.
- * We can override the _DSD to correct the boost type here.
- * Since this laptop has valid ACPI, we do not need to handle cs-gpios, since that already exists
- * in the ACPI.
- */
-static int hp_vision_acpi_fix(struct cs35l41_hda *cs35l41, struct device *physdev, int id,
-			      const char *hid)
-{
-	struct cs35l41_hw_cfg *hw_cfg = &cs35l41->hw_cfg;
-
-	dev_info(cs35l41->dev, "Adding DSD properties for %s\n", cs35l41->acpi_subsystem_id);
-
-	cs35l41->index = id;
-	cs35l41->channel_index = 0;
-	cs35l41->reset_gpio = gpiod_get_index(physdev, NULL, 1, GPIOD_OUT_HIGH);
-	cs35l41->speaker_id = -ENOENT;
-	hw_cfg->spk_pos = cs35l41->index ? 1 : 0; // right:left
-	hw_cfg->gpio1.func = CS35L41_NOT_USED;
-	hw_cfg->gpio1.valid = true;
-	hw_cfg->gpio2.func = CS35L41_INTERRUPT;
-	hw_cfg->gpio2.valid = true;
-	hw_cfg->bst_type = CS35L41_INT_BOOST;
-	hw_cfg->bst_ind = 1000;
-	hw_cfg->bst_ipk = 4500;
-	hw_cfg->bst_cap = 24;
-	hw_cfg->valid = true;
-
-	return 0;
-}
-
 struct cs35l41_prop_model {
 	const char *hid;
 	const char *ssid;
@@ -84,7 +344,36 @@ struct cs35l41_prop_model {
 static const struct cs35l41_prop_model cs35l41_prop_model_table[] = {
 	{ "CLSA0100", NULL, lenovo_legion_no_acpi },
 	{ "CLSA0101", NULL, lenovo_legion_no_acpi },
-	{ "CSC3551", "103C89C6", hp_vision_acpi_fix },
+	{ "CSC3551", "103C89C6", generic_dsd_config },
+	{ "CSC3551", "104312AF", generic_dsd_config },
+	{ "CSC3551", "10431433", generic_dsd_config },
+	{ "CSC3551", "10431463", generic_dsd_config },
+	{ "CSC3551", "10431473", generic_dsd_config },
+	{ "CSC3551", "10431483", generic_dsd_config },
+	{ "CSC3551", "10431493", generic_dsd_config },
+	{ "CSC3551", "104314D3", generic_dsd_config },
+	{ "CSC3551", "104314E3", generic_dsd_config },
+	{ "CSC3551", "10431503", generic_dsd_config },
+	{ "CSC3551", "10431533", generic_dsd_config },
+	{ "CSC3551", "10431573", generic_dsd_config },
+	{ "CSC3551", "10431663", generic_dsd_config },
+	{ "CSC3551", "104316D3", generic_dsd_config },
+	{ "CSC3551", "104316F3", generic_dsd_config },
+	{ "CSC3551", "104317F3", generic_dsd_config },
+	{ "CSC3551", "10431863", generic_dsd_config },
+	{ "CSC3551", "104318D3", generic_dsd_config },
+	{ "CSC3551", "10431C9F", generic_dsd_config },
+	{ "CSC3551", "10431CAF", generic_dsd_config },
+	{ "CSC3551", "10431CCF", generic_dsd_config },
+	{ "CSC3551", "10431CDF", generic_dsd_config },
+	{ "CSC3551", "10431CEF", generic_dsd_config },
+	{ "CSC3551", "10431D1F", generic_dsd_config },
+	{ "CSC3551", "10431DA2", generic_dsd_config },
+	{ "CSC3551", "10431E02", generic_dsd_config },
+	{ "CSC3551", "10431EE2", generic_dsd_config },
+	{ "CSC3551", "10431F12", generic_dsd_config },
+	{ "CSC3551", "10431F1F", generic_dsd_config },
+	{ "CSC3551", "10431F62", generic_dsd_config },
 	{}
 };
 
@@ -97,7 +386,7 @@ int cs35l41_add_dsd_properties(struct cs35l41_hda *cs35l41, struct device *physd
 		if (!strcmp(model->hid, hid) &&
 		    (!model->ssid ||
 		     (cs35l41->acpi_subsystem_id &&
-		      !strcmp(model->ssid, cs35l41->acpi_subsystem_id))))
+		      !strcasecmp(model->ssid, cs35l41->acpi_subsystem_id))))
 			return model->add_prop(cs35l41, physdev, id, hid);
 	}
 
diff --git a/sound/pci/hda/hda_component.h b/sound/pci/hda/hda_component.h
index f170aec967c1..bbd6f0ed16c1 100644
--- a/sound/pci/hda/hda_component.h
+++ b/sound/pci/hda/hda_component.h
@@ -6,6 +6,7 @@
  *                    Cirrus Logic International Semiconductor Ltd.
  */
 
+#include <linux/acpi.h>
 #include <linux/component.h>
 
 #define HDA_MAX_COMPONENTS	4
@@ -15,6 +16,9 @@ struct hda_component {
 	struct device *dev;
 	char name[HDA_MAX_NAME_SIZE];
 	struct hda_codec *codec;
+	struct acpi_device *adev;
+	bool acpi_notifications_supported;
+	void (*acpi_notify)(acpi_handle handle, u32 event, struct device *dev);
 	void (*pre_playback_hook)(struct device *dev, int action);
 	void (*playback_hook)(struct device *dev, int action);
 	void (*post_playback_hook)(struct device *dev, int action);
diff --git a/sound/pci/hda/patch_realtek.c b/sound/pci/hda/patch_realtek.c
index 0db9326b6f84..f747fcae24bb 100644
--- a/sound/pci/hda/patch_realtek.c
+++ b/sound/pci/hda/patch_realtek.c
@@ -9981,22 +9981,28 @@ static const struct snd_pci_quirk alc269_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x1043, 0x1313, "Asus K42JZ", ALC269VB_FIXUP_ASUS_MIC_NO_PRESENCE),
 	SND_PCI_QUIRK(0x1043, 0x13b0, "ASUS Z550SA", ALC256_FIXUP_ASUS_MIC),
 	SND_PCI_QUIRK(0x1043, 0x1427, "Asus Zenbook UX31E", ALC269VB_FIXUP_ASUS_ZENBOOK),
-	SND_PCI_QUIRK(0x1043, 0x1433, "ASUS GX650P", ALC285_FIXUP_ASUS_I2C_HEADSET_MIC),
-	SND_PCI_QUIRK(0x1043, 0x1463, "Asus GA402X", ALC285_FIXUP_ASUS_I2C_HEADSET_MIC),
-	SND_PCI_QUIRK(0x1043, 0x1473, "ASUS GU604V", ALC285_FIXUP_ASUS_HEADSET_MIC),
-	SND_PCI_QUIRK(0x1043, 0x1483, "ASUS GU603V", ALC285_FIXUP_ASUS_HEADSET_MIC),
-	SND_PCI_QUIRK(0x1043, 0x1493, "ASUS GV601V", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1433, "ASUS GX650PY/PZ/PV/PU/PYV/PZV/PIV/PVV", ALC285_FIXUP_ASUS_I2C_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1463, "Asus GA402X/GA402N", ALC285_FIXUP_ASUS_I2C_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1473, "ASUS GU604VI/VC/VE/VG/VJ/VQ/VU/VV/VY/VZ", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1483, "ASUS GU603VQ/VU/VV/VJ/VI", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1493, "ASUS GV601VV/VU/VJ/VQ/VI", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x14d3, "ASUS G614JY/JZ/JG", ALC245_FIXUP_CS35L41_SPI_2),
+	SND_PCI_QUIRK(0x1043, 0x14e3, "ASUS G513PI/PU/PV", ALC287_FIXUP_CS35L41_I2C_2),
+	SND_PCI_QUIRK(0x1043, 0x1503, "ASUS G733PY/PZ/PZV/PYV", ALC287_FIXUP_CS35L41_I2C_2),
 	SND_PCI_QUIRK(0x1043, 0x1517, "Asus Zenbook UX31A", ALC269VB_FIXUP_ASUS_ZENBOOK_UX31A),
-	SND_PCI_QUIRK(0x1043, 0x1533, "ASUS GV302XA", ALC287_FIXUP_CS35L41_I2C_2),
-	SND_PCI_QUIRK(0x1043, 0x1573, "ASUS GZ301V", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1533, "ASUS GV302XA/XJ/XQ/XU/XV/XI", ALC287_FIXUP_CS35L41_I2C_2),
+	SND_PCI_QUIRK(0x1043, 0x1573, "ASUS GZ301VV/VQ/VU/VJ/VA/VC/VE/VVC/VQC/VUC/VJC/VEC/VCC", ALC285_FIXUP_ASUS_HEADSET_MIC),
 	SND_PCI_QUIRK(0x1043, 0x1662, "ASUS GV301QH", ALC294_FIXUP_ASUS_DUAL_SPK),
-	SND_PCI_QUIRK(0x1043, 0x1663, "ASUS GU603ZV", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1663, "ASUS GU603ZI/ZJ/ZQ/ZU/ZV", ALC285_FIXUP_ASUS_HEADSET_MIC),
 	SND_PCI_QUIRK(0x1043, 0x1683, "ASUS UM3402YAR", ALC287_FIXUP_CS35L41_I2C_2),
 	SND_PCI_QUIRK(0x1043, 0x16b2, "ASUS GU603", ALC289_FIXUP_ASUS_GA401),
+	SND_PCI_QUIRK(0x1043, 0x16d3, "ASUS UX5304VA", ALC245_FIXUP_CS35L41_SPI_2),
 	SND_PCI_QUIRK(0x1043, 0x16e3, "ASUS UX50", ALC269_FIXUP_STEREO_DMIC),
+	SND_PCI_QUIRK(0x1043, 0x16f3, "ASUS UX7602VI/BZ", ALC245_FIXUP_CS35L41_SPI_2),
 	SND_PCI_QUIRK(0x1043, 0x1740, "ASUS UX430UA", ALC295_FIXUP_ASUS_DACS),
 	SND_PCI_QUIRK(0x1043, 0x17d1, "ASUS UX431FL", ALC294_FIXUP_ASUS_DUAL_SPK),
-	SND_PCI_QUIRK(0x1043, 0x17f3, "ROG Ally RC71L_RC71L", ALC294_FIXUP_ASUS_ALLY),
+	SND_PCI_QUIRK(0x1043, 0x17f3, "ROG Ally NR2301L/X", ALC294_FIXUP_ASUS_ALLY),
+	SND_PCI_QUIRK(0x1043, 0x1863, "ASUS UX6404VI/VV", ALC245_FIXUP_CS35L41_SPI_2),
 	SND_PCI_QUIRK(0x1043, 0x1881, "ASUS Zephyrus S/M", ALC294_FIXUP_ASUS_GX502_PINS),
 	SND_PCI_QUIRK(0x1043, 0x18b1, "Asus MJ401TA", ALC256_FIXUP_ASUS_HEADSET_MIC),
 	SND_PCI_QUIRK(0x1043, 0x18d3, "ASUS UM3504DA", ALC294_FIXUP_CS35L41_I2C_2),
@@ -10021,10 +10027,13 @@ static const struct snd_pci_quirk alc269_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x1043, 0x1c43, "ASUS UX8406MA", ALC245_FIXUP_CS35L41_SPI_2),
 	SND_PCI_QUIRK(0x1043, 0x1c62, "ASUS GU603", ALC289_FIXUP_ASUS_GA401),
 	SND_PCI_QUIRK(0x1043, 0x1c92, "ASUS ROG Strix G15", ALC285_FIXUP_ASUS_G533Z_PINS),
-	SND_PCI_QUIRK(0x1043, 0x1c9f, "ASUS G614JI", ALC285_FIXUP_ASUS_HEADSET_MIC),
-	SND_PCI_QUIRK(0x1043, 0x1caf, "ASUS G634JYR/JZR", ALC285_FIXUP_ASUS_SPI_REAR_SPEAKERS),
+	SND_PCI_QUIRK(0x1043, 0x1c9f, "ASUS G614JU/JV/JI", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1caf, "ASUS G634JY/JZ/JI/JG", ALC285_FIXUP_ASUS_SPI_REAR_SPEAKERS),
 	SND_PCI_QUIRK(0x1043, 0x1ccd, "ASUS X555UB", ALC256_FIXUP_ASUS_MIC),
-	SND_PCI_QUIRK(0x1043, 0x1d1f, "ASUS ROG Strix G17 2023 (G713PV)", ALC287_FIXUP_CS35L41_I2C_2),
+	SND_PCI_QUIRK(0x1043, 0x1ccf, "ASUS G814JU/JV/JI", ALC245_FIXUP_CS35L41_SPI_2),
+	SND_PCI_QUIRK(0x1043, 0x1cdf, "ASUS G814JY/JZ/JG", ALC245_FIXUP_CS35L41_SPI_2),
+	SND_PCI_QUIRK(0x1043, 0x1cef, "ASUS G834JY/JZ/JI/JG", ALC285_FIXUP_ASUS_HEADSET_MIC),
+	SND_PCI_QUIRK(0x1043, 0x1d1f, "ASUS G713PI/PU/PV/PVN", ALC287_FIXUP_CS35L41_I2C_2),
 	SND_PCI_QUIRK(0x1043, 0x1d42, "ASUS Zephyrus G14 2022", ALC289_FIXUP_ASUS_GA401),
 	SND_PCI_QUIRK(0x1043, 0x1d4e, "ASUS TM420", ALC256_FIXUP_ASUS_HPE),
 	SND_PCI_QUIRK(0x1043, 0x1da2, "ASUS UP6502ZA/ZD", ALC245_FIXUP_CS35L41_SPI_2),
@@ -10040,6 +10049,7 @@ static const struct snd_pci_quirk alc269_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x1043, 0x1c52, "ASUS Zephyrus G15 2022", ALC289_FIXUP_ASUS_GA401),
 	SND_PCI_QUIRK(0x1043, 0x1f11, "ASUS Zephyrus G14", ALC289_FIXUP_ASUS_GA401),
 	SND_PCI_QUIRK(0x1043, 0x1f12, "ASUS UM5302", ALC287_FIXUP_CS35L41_I2C_2),
+	SND_PCI_QUIRK(0x1043, 0x1f1f, "ASUS H7604JI/JV/J3D", ALC245_FIXUP_CS35L41_SPI_2),
 	SND_PCI_QUIRK(0x1043, 0x1f62, "ASUS UX7602ZM", ALC245_FIXUP_CS35L41_SPI_2),
 	SND_PCI_QUIRK(0x1043, 0x1f92, "ASUS ROG Flow X16", ALC289_FIXUP_ASUS_GA401),
 	SND_PCI_QUIRK(0x1043, 0x3030, "ASUS ZN270IE", ALC256_FIXUP_ASUS_AIO_GPIO2),
